(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "08B0-1D1T-06-F" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 44.45 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "08B0-1D1T-06-F" (at 44.45 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "08B01D1T06F" (at 44.45 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://datasheet.datasheetarchive.com/originals/distributors/Datasheets_SAMA/2324c65ca93fd072f187737ff3c96afb.pdf" (at 44.45 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "Conn RJ-45 F 6 POS 2.03mm Solder RA Thru-Hole 10 Terminal 1 Port Tray" (at 44.45 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "13.49" (at 44.45 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "" (at 44.45 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "" (at 44.45 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "BelFuse" (at 44.45 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "08B0-1D1T-06-F" (at 44.45 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 43.18 -15.24)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "TCT" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "TD+" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "TD-" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "RD+" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "RD-" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "RCT" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 48.26 0 180) (length 5.08)
      (name "CATHODE_LED_1_GREEN" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 48.26 -2.54 180) (length 5.08)
      (name "ANODE_LED_1_GREEN" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 48.26 -5.08 180) (length 5.08)
      (name "CATHODE_LED_2_YELLOW" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 48.26 -7.62 180) (length 5.08)
      (name "ANODE_LED_2_YELLOW" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 48.26 -10.16 180) (length 5.08)
      (name "MH3" (effects (font (size 1.27 1.27))))
      (number "MH3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 48.26 -12.7 180) (length 5.08)
      (name "MH4" (effects (font (size 1.27 1.27))))
      (number "MH4" (effects (font (size 1.27 1.27))))
    )
  )
)
