(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "XR32330EBERTR-F" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 25.4 10.16 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "XR32330EBERTR-F" (id 1) (at 25.4 7.62 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "QFN-24" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "XR32330EBERTR-F" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "XR32330EBERTR-F" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN-24 QFN-24-M QFN-24-L" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "XR32330EBERTR-F_0_1"
      (polyline
        (pts
          (xy 7.62 5.08)
          (xy 7.62 -35.56)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 -35.56)
          (xy 43.18 -35.56)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 43.18 -35.56)
          (xy 43.18 5.08)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 43.18 5.08)
          (xy 7.62 5.08)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin input line (at 0 0 0) (length 7.62)
        (name "R1IN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -2.54 0) (length 7.62)
        (name "R2IN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 7.62)
        (name "R3IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -7.62 0) (length 7.62)
        (name "T1OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -10.16 0) (length 7.62)
        (name "T2OUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -12.7 0) (length 7.62)
        (name "T3OUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -15.24 0) (length 7.62)
        (name "T3IN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -17.78 0) (length 7.62)
        (name "T2IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -20.32 0) (length 7.62)
        (name "T1IN" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -22.86 0) (length 7.62)
        (name "R3OUT" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -25.4 0) (length 7.62)
        (name "R2OUT" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -27.94 0) (length 7.62)
        (name "R1OUT" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 50.8 -30.48 180) (length 7.62)
        (name "*STATUS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 50.8 -27.94 180) (length 7.62)
        (name "*SHUTDOWN" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 50.8 -25.4 180) (length 7.62)
        (name "*ONLINE" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 50.8 -22.86 180) (length 7.62)
        (name "C1-" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 50.8 -20.32 180) (length 7.62)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 50.8 -17.78 180) (length 7.62)
        (name "VL" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 50.8 -15.24 180) (length 7.62)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 50.8 -12.7 180) (length 7.62)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 50.8 -10.16 180) (length 7.62)
        (name "C1+" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 50.8 -7.62 180) (length 7.62)
        (name "C2+" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 50.8 -5.08 180) (length 7.62)
        (name "C2-" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 50.8 -2.54 180) (length 7.62)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 50.8 0 180) (length 7.62)
        (name "EPAD" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
    )
  )
)

