<?xml version="1.0" encoding="utf-8"?>
<!--/2118843/1015067/2.50/6/2/Connector/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Body Features: Primary Product Color White | Configuration Features: PCB Mount Orientation Right Angle | Compatible With Wire &amp; Cable Type FPC | Number of Rows 1 | Compatible With Wire &amp; Cable Type FFC | Number of Positions 6 | Contact Features: Contact Mating Location Top | PCB Contact Termination Area Plating Material Finish Bright | Contact Mating Area Plating Material Finish Bright | Contact Type Socket | PCB Contact Termination Area Plating Material Thickness .8 MICM | Contact Mating Area Plating Mater&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="845336">
<description>&lt;b&gt;84533-6-4&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="84533-6">
<pin name="1" direction="io"/>
<pin name="2" direction="io"/>
<pin name="3" direction="io"/>
<pin name="4" direction="io"/>
<pin name="5" direction="io"/>
<pin name="6" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="84533-6" prefix="J">
<description>&lt;b&gt;Body Features: Primary Product Color White | Configuration Features: PCB Mount Orientation Right Angle | Compatible With Wire &amp; Cable Type FPC | Number of Rows 1 | Compatible With Wire &amp; Cable Type FFC | Number of Positions 6 | Contact Features: Contact Mating Location Top | PCB Contact Termination Area Plating Material Finish Bright | Contact Mating Area Plating Material Finish Bright | Contact Type Socket | PCB Contact Termination Area Plating Material Thickness .8 MICM | Contact Mating Area Plating Mater&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&amp;DocId=Customer Drawing84533E1pdfEnglishENG_CD_84533_E1.pdf84533-6"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="84533-6"/>
</gates>
<devices>
<device name="" package="845336">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="571-84533-6"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity-AMP/84533-6?qs=%252BtLcN0raKGXizCLpBiKXdA%3D%3D"/>
<attribute name="Manufacturer_Name" value="TE Connectivity"/>
<attribute name="Manufacturer_Part_Number" value="84533-6"/>
<attribute name="Description" value="Body Features: Primary Product Color White | Configuration Features: PCB Mount Orientation Right Angle | Compatible With Wire &amp; Cable Type FPC | Number of Rows 1 | Compatible With Wire &amp; Cable Type FFC | Number of Positions 6 | Contact Features: Contact Mating Location Top | PCB Contact Termination Area Plating Material Finish Bright | Contact Mating Area Plating Material Finish Bright | Contact Type Socket | PCB Contact Termination Area Plating Material Thickness .8 MICM | Contact Mating Area Plating Mater"/>
<attribute name="Height" value="5.05mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
